Installation Requirements

* Latitude Tilt (~14 deg for North Philippines)
* Facing south

Strength Requirements

* 300 kph wind

Durability Requirements

* 10 years
* 25 year lifetime of panel

House Safety

* High winds on the panel shouldn’t break the house
* Oscillating…

Taobao